**SPECIFICATION TABLE**

|  |  |  |  |
| --- | --- | --- | --- |
|  | **Galaxy A56 5G** | **Galaxy A36 5G** | **Galaxy A26 5G** |
| **Display** | 6.7-inch FHD+ | | |
| Super AMOLED Display  Up to 120Hz refresh rate  Vision Booster | | |
| \*Measured diagonally, the screen size is 6.7-inch in the full rectangle and 6.5-inch with accounting for the rounded corners; actual viewable area is less due to the rounded corners and camera hole. | | |
| **Dimensions & Weight** | 162.2 x 77.5 x 7.4mm, 198g | 162.9 x 78.2 x 7.4mm, 195g | 164.0 x 77.5 x 7.7mm, 200g |
| \*Device weight may vary by market. | | |
| **Camera** | 12MP Ultra-Wide Camera   * F2.2   50MP Main Camera   * F1.8, AF, OIS   5MP Macro Camera   * F2.4   12MP Front Camera   * F2.2 | 8MP Ultra-Wide Camera   * F2.2   50MP Main Camera   * F1.8, AF, OIS   5MP Macro Camera   * F2.4   12MP Front Camera   * F2.2 | 8MP Ultra-Wide Camera   * F2.2   50MP Main Camera   * F1.8, AF, OIS   2MP Macro Camera   * F2.4   13MP Front Camera   * F2.2 |
| **Memory & Storage** | 8GB + 128GB  8GB + 256GB  12GB + 256GB | 6GB + 128GB  8GB + 128GB  8GB + 256GB  12GB + 256GB | 6GB + 128GB  8GB + 128GB  8GB + 256GB |
| \*Storage options and availability may vary by carrier, market or region. Actual storage availability may vary depending on pre-installed software. | | |
| **Battery** | 5,000mAh (typical) | | |
| \*Typical value tested under third-party laboratory conditions. Typical value is the estimated average value considering the deviation in battery capacity among the battery samples tested under IEC 61960 standard. Rated (minimum) capacity is 4,905mAh. Actual battery life may vary depending on network environment, usage patterns and other factors. | | |
| **OS** | Android 15 | | |
| One UI 7 | | |
| **Security** | Samsung Knox | | |
| **Water & Dust Resistance** | IP67[[1]](#footnote-1) | | |

\*Specifications may vary by market.  
\*All functionality, features, specifications and other product information provided in this document including, but not limited to, the benefits, design, pricing, components, performance, availability, and capabilities of the product are subject to change without notice.

1. IP67-klassificeringen er baseret på laboratorietests under forhold, hvor enheden er nedsænket i op til 1 meter ferskvand i maksimalt 30 minutter. Anbefales ikke til brug på stranden, i poolen eller i sæbevand. Enhedens vand- og støvmodstand er ikke permanent og kan aftage over tid [↑](#footnote-ref-1)