****

**M12 connectors with push-pull locking**

# Phoenix Contact is extending its portfolio of M12 connectors with push-pull fast locking system: the A-, D-, and L-coded device connectors with pin contacts are available with the appropriate push-pull housing screw connections for SMD and THR processes. Alternatively, there are also versions for wave soldering.

# The push-pull device plugs with pre-assembled litz wires are suitable for longer distances inside the device. The corresponding field connectors for assembly intended for signal transmission (A-coded) and for data transmission in accordance with CAT5 (D-coded) have crimp connections for conductor cross sections up to 0.34 mm² or 1 mm².

# The fast locking system works without tools, simply by plugging in. The user receives clear feedback of secure connection: the mechanism springs back when the connectors are not snapped into place properly. The cross-manufacturer compatibility of this principle ensures high availability worldwide.

**ENDS**

# PR5205GB

April 2020

Phoenix Contact Ltd

Halesfield 13

Telford

Shropshire

TF7 4PG

Tel: 0845 881 2222

Fax: 0845 881 2211

[www.phoenixcontact.co.uk](http://www.phoenixcontact.co.uk)

info@phoenixcontact.co.uk

**For news updates from Phoenix Contact visit:**

**Phoenix Contact Press Room** – http://www.mynewsdesk.com/uk/phoenix-contact-uk

**Twitter** - @phoenixcontactu

**YouTube** – Phoenix Contact UK

**Blog** – www.phoenixcontact.co.uk/blog

**LinkedIn** – www.linkedin.com/company/phoenix-contact-uk

For further information on this press release please contact:

Phoenix Contact Ltd, Halesfield 13, Telford, TF7 4PG.

marketing@phoenixcontact.co.uk