******Compact connectors for LED PCBs**

With the new connectors from the PTF series from Phoenix Contact, you can quickly and easily connect flexible LED PCBs.

Secure press fit connection: the new PTF series of direct connectors can be used to connect 10 mm wide LED PCBs easily and reliably. The integrated locking mechanism ensures a secure and permanent connection with the PCB. The compact connectors are designed for currents up to 10 A and voltages up to 24 V (UL: 50 V). Thanks to their compact size, they are also suitable for applications in confined spaces such as narrow linear profiles.

The product range now comprises 2 and 4-pos. feed-in elements and butt connectors in the pitches 1.9 mm for 8 mm wide PCBs and 2.4 mm for 10 mm wide PCBs. At just 4.2 mm high, the white direct connectors were developed according to IEC 60838-2-2. They are suitable for various LED applications in building or ambient lighting.

**ENDS**

**March 2016**

**PR4816GB**

Phoenix Contact Ltd

Halesfield 13

Telford

Shropshire

TF7 4PG

Tel: 0845 881 2222

Fax: 0845 881 2211

[www.phoenixcontact.co.uk](http://www.phoenixcontact.co.uk)

info@phoenixcontact.co.uk

**For news updates from Phoenix Contact visit:**

**Phoenix Contact Press Room** – http://www.mynewsdesk.com/uk/phoenix-contact-uk

**Twitter** - @phoenixcontactu

**YouTube** – Phoenix Contact UK

**Blog** – www.phoenixcontact.co.uk/blog

**LinkedIn** – www.linkedin.com/company/phoenix-contact-uk