******Connector housing with lateral and straight cable outlet direction**

Phoenix Contact now has now expanded the range of Heavycon Evo heavy-duty industrial connectors by three Twin housings. The housings are available in the sizes B10 to B24 for double locking latches with two differently marked cable inlets.

The matching cable glands with bayonet locking in the sizes M20 to M40 allow both lateral and direct cable outlet direction with one housing. Particularly for modular contact inserts, where various cables for signals, data, power, and pneumatics must be frequently routed through a connector housing, the TWIN housing is an alternative to protective hoses or special housings with individual cable inlets.

With comparably few individual parts, the system provides a high degree of flexibility of cable inlet and cable outlet directions. Furthermore, it is possible to subsequently adapt the cable outlet directions on site. The housing material is specified for extreme industrial conditions. The housings fulfil the requirements according to IP65/66 degree of protection.

**ENDS**

**September 2015**

**PR4786GB**

Phoenix Contact Ltd

Halesfield 13

Telford

Shropshire

TF7 4PG

Tel: 0845 881 2222

Fax: 0845 881 2211

[www.phoenixcontact.co.uk](http://www.phoenixcontact.co.uk)

info@phoenixcontact.co.uk

**For news updates from Phoenix Contact visit:**

**Phoenix Contact Press Room** – http://www.mynewsdesk.com/uk/phoenix-contact-uk

**Twitter** - @phoenixcontactu

**YouTube** – Phoenix Contact UK

**Blog** – www.phoenixcontact.co.uk/blog

**LinkedIn** – www.linkedin.com/company/phoenix-contact-uk