******Y-distributor separates CAT5 and power**

A Y-coded interface can transmit both data and power and also reduces the number of cables in the system. The new Y-coded Y-distributor from Phoenix Contact enables the easy integration of devices with hybrid M12 interfaces.

It has a Y-coded interface on one side and an A and D-coded interface on the other side. CAT5 requirements are therefore satisfied. This means that new sensors can also be integrated into existing cabling. A and D-coded standard cables that are already in use can be retained. The Speedcon fast locking system reduces assembly time.

**ENDS**

**July 2016**

**PR4880GB**

Phoenix Contact Ltd

Halesfield 13

Telford

Shropshire

TF7 4PG

Tel: 0845 881 2222

Fax: 0845 881 2211

[www.phoenixcontact.co.uk](http://www.phoenixcontact.co.uk)

[info@phoenixcontact.co.uk](mailto:info@phoenixcontact.co.uk)

**For news updates from Phoenix Contact visit:**

**Phoenix Contact Press Room** – http://www.mynewsdesk.com/uk/phoenix-contact-uk

**Twitter** - @phoenixcontactu

**YouTube** – Phoenix Contact UK

**Blog** – www.phoenixcontact.co.uk/blog

**LinkedIn** – www.linkedin.com/company/phoenix-contact-uk