******

**Compact AC connection for photovoltaic micro inverters**

The new SUNCLIX Micon AC connection system from Phoenix Contact reliably connects photovoltaic modules. The system, which consists of Y-connectors and the matching mains connectors, is so compact that it can be easily installed behind the module frame. The components offer IP67 protection and are suitable for temperature ranges from -40°C to +90°C.

The cables assembled according to customer requests are ideal for currents up to 20 A as well as voltages up to 600 V. In addition to the versions with European certification in cross sections from 0.75 mm2 (branch lines) and 2.5 mm2 (trunk lines), the AWG18 and AWG12 conductor cross sections are also available for the North American market.

Ends

July 2014

**PR4646GB**

Phoenix Contact Ltd

Halesfield 13

Telford

Shropshire

TF7 4PG

Tel: 0845 881 2222

Fax: 0845 881 2211

[www.phoenixcontact.co.uk](http://www.phoenixcontact.co.uk)

[info@phoenixcontact.co.uk](mailto:info@phoenixcontact.co.uk)