********Highly compact signal conditioners listed by UL**

Mini Analog Pro highly compact signal conditioners with plug-in connection technology from Phoenix Contact are now listed for the USA and Canada in accordance with UL 508.

The 6 mm signal conditioner range with plug-in connection technology offers easy installation and startup in a confined space. Easily visible and accessible terminal points and current measurement during operation make work easier. Many device types can be configured for individual adaptation to the respective application: from simple DIP switch configuration to advanced configuration via software or smart-phone app without additional accessories.

Despite the compact design, large-surface marking areas enable complete loop identification. Status LEDs in every signal conditioner and group error indication via the DIN rail connector ensure quick and consistent diagnostics.

Furthermore, the signal conditioners offer high signal quality, thanks to the latest transmission technology and safe electrical isolation with 3 kV test voltage. The extended supply voltage range of 9.6 V DC to 30 V DC and the wide operating temperature range of -40°C to +70°C open up a wide range of possible applications.

Ends

July 2014

**PR4649GB**

Phoenix Contact Ltd

Halesfield 13

Telford

Shropshire

TF7 4PG

Tel: 0845 881 2222

Fax: 0845 881 2211

[www.phoenixcontact.co.uk](http://www.phoenixcontact.co.uk)

[info@phoenixcontact.co.uk](mailto:info@phoenixcontact.co.uk)