******Assembled M12 POWER cabling in M-coding**

# The new Phoenix Contact power cables achieve high performance in a compact design. The assembled M12 POWER cables with M-coded connectors are ideal for AC applications up to 8 A and 690 V. The coded pin connector pattern offers protection against incorrect connections.

# In addition to three phases plus PE, two additional contacts are available that can be used for a motor brake, for example. An optional 360° shielding offers reliable EMC protection. The compact design of the M12 connectors ensures space savings for power cabling.

**ENDS**

**Sept 2018**

**PR5068GB**

Phoenix Contact Ltd

Halesfield 13

Telford

Shropshire

TF7 4PG

Tel: 0845 881 2222

Fax: 0845 881 2211

[www.phoenixcontact.co.uk](http://www.phoenixcontact.co.uk)

[info@phoenixcontact.co.uk](mailto:info@phoenixcontact.co.uk)

**For news updates from Phoenix Contact visit:**

**Phoenix Contact Press Room** – http://www.mynewsdesk.com/uk/phoenix-contact-uk

**Twitter** - @phoenixcontactu

**YouTube** – Phoenix Contact UK

**Blog** – www.phoenixcontact.co.uk/blog

**LinkedIn** – www.linkedin.com/company/phoenix-contact-uk