***Press Release***

**High conductor pull-out values with square crimping shape**

# The Crimpfox Vario 4S crimping tool from Phoenix Contact ensures reliable processing of insulated, uninsulated, and TWIN ferrules.

# The integrated pressure lock guarantees a complete and process-reliable crimping cycle and, when necessary, can be released without using a special tool.

# The tool’s self-adjusting crimping jaw enables the processing of ferrules in accordance with DIN 46228-1 and -4 and with special collars in the cross-section range from 0.25 to 4 mm² as well as TWIN ferrules up to 2 x 1.5 mm² without having to make adjustments. In addition, the crimping tool supports a cross-section range from 6 to 10 mm² and 16 mm². The special square crimping shape results in maximum possible contact surfaces and high conductor pull-out values, which are therefore also ideal for spring connection technology.

# Ends

# PR5267GB

October 2020

Phoenix Contact Ltd

Halesfield 13

Telford

Shropshire

TF7 4PG

Tel: 0845 881 2222

Fax: 0845 881 2211

[www.phoenixcontact.co.uk](http://www.phoenixcontact.co.uk)

[info@phoenixcontact.co.uk](mailto:info@phoenixcontact.co.uk)

**For news updates from Phoenix Contact visit:**

**Phoenix Contact Press Room** – http://www.mynewsdesk.com/uk/phoenix-contact-uk

**Twitter** - @phoenixcontactu

**Blog** – www.phoenixcontact.co.uk/blog

**LinkedIn** – www.linkedin.com/company/phoenix-contact-uk

For further information on this press release please contact:

Phoenix Contact Ltd, Halesfield 13, Telford, TF7 4PG.

marketing@phoenixcontact.co.uk