**Feed-through connectors with 5.08 mm pitch**

# Phoenix Contact is introducing new feed-through connectors with 5.08 mm pitch to the market. The inverted connectors with screw connection are designed for conductor cross sections from 0.2 to 2.5 mm² and enable flying leads though the device panel.

# The DFK-MSTB series is compatible with MSTB and FKC series connectors without flange, with screw flange, and with Lock and Release locking. The 2- to 16-pos. versions can transmit currents up to 12 A and voltages up to 320 V, and are suitable for a panel thickness of up to 5 mm.

**ENDS**

# PR5202GB

July 2020

Phoenix Contact Ltd

Halesfield 13

Telford

Shropshire

TF7 4PG

Tel: 0845 881 2222

Fax: 0845 881 2211

[www.phoenixcontact.co.uk](http://www.phoenixcontact.co.uk)

[info@phoenixcontact.co.uk](mailto:info@phoenixcontact.co.uk)

**For news updates from Phoenix Contact visit:**

**Phoenix Contact Press Room** – http://www.mynewsdesk.com/uk/phoenix-contact-uk

**Twitter** - @phoenixcontactu

**YouTube** – Phoenix Contact UK

**Blog** – www.phoenixcontact.co.uk/blog

**LinkedIn** – www.linkedin.com/company/phoenix-contact-uk

For further information on this press release please contact:

Phoenix Contact Ltd, Halesfield 13, Telford, TF7 4PG.

marketing@phoenixcontact.co.uk