********Space savings across three levels**

The new UT 4-PE/L/HESI fuse terminal block range with screw connection from Phoenix Contact offers a high degree of functionality on three levels with a pitch of just 6.2 mm. The double bridge shaft on each level allows all tasks for potential in-feed and distribution to be implemented quickly and easily.

For switching tasks, especially in MCR technology, an isolating plug, feed-through metal, component connector for the solder-free installation of electronic components or a fuse plug for 5 x 20 and 6.3 x 32 glass tube fuses can be used in the disconnect zone of the disconnect terminal blocks depending on the application. Feed-through terminal blocks of the same shape complete the range.

All modular terminal blocks in the UT screw terminal block series use the cross-system accessories of the Clipline complete modular terminal block system. In addition to using the same bridge system, marking and testing is identical for push-in, spring-cage, COMBI, and IDC fast connection technology.

**Ends**

**Jul 2014**

**PR4661GB**

Phoenix Contact Ltd

Halesfield 13

Telford

Shropshire

TF7 4PG

Tel: 0845 881 2222

Fax: 0845 881 2211

[www.phoenixcontact.co.uk](http://www.phoenixcontact.co.uk)

info@phoenixcontact.co.uk