TECHNICAL DATA SHEET

**Dimensions**

|  |  |  |
| --- | --- | --- |
| **TRUNK VOLUME** | **All versions except full hybrid** | **Full Hybrid Version** |
| **With row 2 moved forward / moved back to stop (+ 132L) in litres** | **484 / 616** | **348 / 480** |
| **With row 2 advanced / retracted to stop (+ 114 dm3) in VDA standard dm3** | **422 / 536** | **326 / 440** |
| **Maximum volume (up to the height of the seat) - rear bench folded down** | **1 596** | **1 458** |

|  |  |
| --- | --- |
| **DIMENSIONS (mm)** |  |
| **Overhall lenght** | **4 239** |
| **Wheelbase** | **2 639** |
| **Front overhang** | **883** |
| **Rear overhang** | **717** |
| **Overall width with folded mirrors / unfolded mirrors** | **1 797 / 2 003** |
| **Front track ground** | **1 562** |
| **Rear track ground** | **1 547** |
| **Overall height without/with longitudinal roof bars** | **1 575** |
| **Open tailgate height** | **2 044** |
| **Trunk sill height** | **779** |
| **Ground clearance unladen / with max. load** | **169 / 132** |
| **Rear Knee radius row 2 advanced / retracted to stop** | **61 / 221** |
| **Front elbow room** | **1 396** |
| **Rear elbow room** | **1390** |
| **Front shoulder width** | **1371** |
| **Rear shoulder width** | **1340** |
| **Front headroom** | **889 / 879 - 939 / 929** |
| **Rear headroom** | **849 / 849 - 906 / 908** |
| **Trunk entry maximum width** | **953** |
| **Interior width between wheel arches** | **976** |
| **Maximum load length with rear bench folded** | **1 571** |

**Powertrain characteristics**

|  |  |
| --- | --- |
|  | **RENAULT CAPTUR** |
| **Powertrain** | **1.0 TCE 90**  | **1.0 TCE 100 LPG** | **1.3 TCE 140 mild hybrid** | **1.3 TCE 155** | **1.3 TCE 160 mild hybrid**  | **E-Tech full hybrid 145** |
| **Fuel**  | Petrol  | Petrol  | Petrol  | Petrol | Petrol  | Petrol |
| **Electification**  | No | No | MH12Costing stop 7kph | No | MH12Costing stop 20kph | HEV 245V |
| **Cylinder Capacity [L]/[cm3]** | 1.0 / 999 | 1.0 / 999 | 1.3 / 1330 | 1.3 / 1330 | 1.3 / 1330 | 1.6 / 1598 |
| **Number of Cylinder** | 3 | 3 | 4 | 4 | 4 | 4 |
| **Number of valves** | 12 | 12 | 16 | 16 | 16 | 16 |
| **Torque [Nm/tr]** | 160 Nm @2750rpm | 160 Nm petrol mode / 2750rpm170Nm LPG mode / 2000rpm | 260 Nm @3500rpm | 270 Nm @1700rpm | 270 Nm @1750rpm | 145 Nm @ 3200rpm ICE mode / 250Nm ICE+EM |
| **Air Alimentation** | Turbo | Turbo  | Turbo  | Turbo | Turbo  | Atmo |
| **CO² gr/km WLTP** | 131 | 119 | 133 | 149 | 133 | 105 |
| **0 to 100 km/h (s)** | 14 | 13 | 10.4 | 8.5 | 8.5 | 10 |
| **Fuel consumption** | 5,8 - 5,9 | 6,0 - 6,1 L with unleaded / 7,7-7,9 L with LPG | 5,8 - 5,9 | 6.2 | 5,8 - 5,9 | 4,7 - 4,9 |