****

**New headers with 7.62 mm pitch**

# The new horizontal and vertical headers from Phoenix Contact with 7.62 mm pitch are specifically tailored to the requirements of power electronics and are compatible with the LPC 6 and PC 6/.. ST-BUS series. Device manufacturers can therefore combine a header type with various connectors and implement devices with different connection technologies.

# The headers are suitable for currents up to 41 A and for voltages up to 1000 V. The two- to six-position versions are available with a middle flange as an option, and provide increased touch protection in the pin connector pattern in accordance with IEC/UL 61800-5-1.

**ENDS**

# PR5201GB

February 2020

Phoenix Contact Ltd

Halesfield 13

Telford

Shropshire

TF7 4PG

Tel: 0845 881 2222

Fax: 0845 881 2211

[www.phoenixcontact.co.uk](http://www.phoenixcontact.co.uk)

[info@phoenixcontact.co.uk](mailto:info@phoenixcontact.co.uk)

**For news updates from Phoenix Contact visit:**

**Phoenix Contact Press Room** – http://www.mynewsdesk.com/uk/phoenix-contact-uk

**Twitter** - @phoenixcontactu

**YouTube** – Phoenix Contact UK

**Blog** – www.phoenixcontact.co.uk/blog

**LinkedIn** – www.linkedin.com/company/phoenix-contact-uk

For further information on this press release please contact:

Phoenix Contact Ltd, Halesfield 13, Telford, TF7 4PG.

marketing@phoenixcontact.co.uk