****

**Double-row PCB connectors**

# Shielded PCB connectors in 2.54mm pitch supplement the existing Phoenix Contact product portfolio. Due to their EMC shielding, the DMCC series double-row connectors enable the reliable supply of data and power to devices – also via a single Ethernet cable (PoE).

# The crimp connectors are suitable for conductor cross sections between 0.14 and 0.75 mm², and are designed for currents up to 6 A/160 V. With their compact size, the 2-pos., four-contact connectors and headers are the solution for applications where space is at a premium. Optional tools enable manual or automated crimping.

# Ends

# PR5200GB

January 2020

Phoenix Contact Ltd

Halesfield 13

Telford

Shropshire

TF7 4PG

Tel: 0845 881 2222

Fax: 0845 881 2211

[www.phoenixcontact.co.uk](http://www.phoenixcontact.co.uk)

info@phoenixcontact.co.uk

**For news updates from Phoenix Contact visit:**

**Phoenix Contact Press Room** – http://www.mynewsdesk.com/uk/phoenix-contact-uk

**Twitter** - @phoenixcontactu

**YouTube** – Phoenix Contact UK

**Blog** – www.phoenixcontact.co.uk/blog

**LinkedIn** – www.linkedin.com/company/phoenix-contact-uk

For further information on this press release please contact:

Phoenix Contact Ltd, Halesfield 13, Telford, TF7 4PG.

marketing@phoenixcontact.co.uk