****

**SKEDD direct connectors with crimp connection**

# Phoenix Contact presents its new double-row direct connectors with crimp connection. The CDDC 1,5 and CDDC 2,5 product series are ideal for applications with a high contact density.

# With SKEDD direct connection technology, the connectors can be connected directly to the printed circuit board without tools and without a header. The CDDC 1,5 series with 3.5 mm pitch is designed for conductor cross sections up to 1.5 mm² and enables currents up to 8 A and voltages up to 160 V. The CDDC 2,5 series with 5.0 mm pitch is suitable for conductor cross sections up to 2.5 mm² and 12 A/320 V. Both variants offer 2- to 16-pos. versions for up to 32 connections.

# Ends

# PR5201GB

February 2020

Phoenix Contact Ltd

Halesfield 13

Telford

Shropshire

TF7 4PG

Tel: 0845 881 2222

Fax: 0845 881 2211

[www.phoenixcontact.co.uk](http://www.phoenixcontact.co.uk)

info@phoenixcontact.co.uk

**For news updates from Phoenix Contact visit:**

**Phoenix Contact Press Room** – http://www.mynewsdesk.com/uk/phoenix-contact-uk

**Twitter** - @phoenixcontactu

**YouTube** – Phoenix Contact UK

**Blog** – www.phoenixcontact.co.uk/blog

**LinkedIn** – www.linkedin.com/company/phoenix-contact-uk

For further information on this press release please contact:

Phoenix Contact Ltd, Halesfield 13, Telford, TF7 4PG.

marketing@phoenixcontact.co.uk