# FlexLink launches X45H, the strong extension of the X45 platform

***Following the successful launch of the X45 conveyor platform in the pharmaceutical and lab automation industries, FlexLink is launching a complementary platform for longer conveyor segments fully compatible to the innovative puck handling functions.***

18 months after the launch of X45, FlexLink has established a position in the lab automation business. In parallel with the business development, FlexLink has developed extensions to the offer and are now launching the new conveyor platform X45H, new puck handling functions and the possibility to connect X45 to X45H.

The new conveyor platform, X45H, is a direct response to customer needs within lab automation. It offers considerably longer conveyor sections and full compatibility to the electro mechanic puck handling functions with embedded controls of the X45*e* platform.

The new X45H platform offers a maximum conveyor length of 25 m and a speed limit of 60 m/min. The conveyor width is 45 mm as the compact X45 platform.

The catalogue and CAD models are available in the Technical library on FlexLink’s web site, www.flexlink.com, under [‘Conveyor system X45’](http://www.flexlink.com/en/Images/5685_X45.pdf).

Göran Abbestam, FlexLink’s product Manager for aluminium based systems explains “The feedback from customers is strong and we have already received orders from several customers within the pharmaceutical and lab automation industries. Our customers within lab automation explicitly express satisfaction about the additional degree of freedom of the layout design the new combined offer is giving them. The development has been made in close cooperation with major integrators.

FlexLink Group

Göran Abbestam Klas Ålander  
Product Manager Corporate Communications   
+46 31 337 1052 +46 31 337 2499

[goran.abbestam@flexlink.com](mailto:goran.abbestam@flexlink.com) [klas.alander@flexlink.com](mailto:klas.alander@flexlink.com)