****

**Compact connector housings for single modular contact inserts**

The new Heavycon EVO M1 plastic housings from Phoenix Contact accommodate a modular contact insert. They are smaller and more cost-effective than a B6 interface. Like all EVO housings, the M1 single-module housings also feature a swivel cable gland with bayonet locking.

In combination with two EVO cable glands, four housing variants can be created from just one sleeve. The cable outlet direction only needs to be defined when the cable gland is snapped on. Simply choose between a side or straight outlet. The panel mounting base and sleeve housing are interlocked via a single locking latch.

The M1 housings are suitable for all standard single modules. Data, signals or power can thus be transmitted conveniently via a single compact interface. The plastic housings meet IP66 degree of protection and are shock-proof up to IK09.

**ENDS**

**August 2018**

**PR5062GB**

Phoenix Contact Ltd

Halesfield 13

Telford

Shropshire

TF7 4PG

Tel: 0845 881 2222

Fax: 0845 881 2211

[www.phoenixcontact.co.uk](http://www.phoenixcontact.co.uk)

[info@phoenixcontact.co.uk](mailto:info@phoenixcontact.co.uk)

**For news updates from Phoenix Contact visit:**

**Phoenix Contact Press Room** – http://www.mynewsdesk.com/uk/phoenix-contact-uk

**Twitter** - @phoenixcontactu

**YouTube** – Phoenix Contact UK

**Blog** – www.phoenixcontact.co.uk/blog

**LinkedIn** – www.linkedin.com/company/phoenix-contact-uk