**Hybrid device connectors with knurled nut**

# M23 Hybrid series device connectors from Phoenix Contact are now also available with a knurled nut. This enables devices such as servo drives to be connected using either coupler or cable connectors. Inputs and outputs can therefore be clearly distinguished – both visually and mechanically. This increases cabling safety, especially in daisy chain applications.

# The hybrid connectors with pin or socket contacts enable the transmission of signals, data, and power in a single connector. A CAT5 data interface or four additional signal contacts are available for this. The device connectors are suitable for currents up to 30 A and voltages up to 630 V AC/850 V DC.

**ENDS**

# PR5206GB

August 2020

Phoenix Contact Ltd

Halesfield 13

Telford

Shropshire

TF7 4PG

Tel: 0845 881 2222

Fax: 0845 881 2211

[www.phoenixcontact.co.uk](http://www.phoenixcontact.co.uk)

info@phoenixcontact.co.uk

**For news updates from Phoenix Contact visit:**

**Phoenix Contact Press Room** – http://www.mynewsdesk.com/uk/phoenix-contact-uk

**Twitter** - @phoenixcontactu

**YouTube** – Phoenix Contact UK

**Blog** – www.phoenixcontact.co.uk/blog

**LinkedIn** – www.linkedin.com/company/phoenix-contact-uk

For further information on this press release please contact:

Phoenix Contact Ltd, Halesfield 13, Telford, TF7 4PG.

marketing@phoenixcontact.co.uk