**Flowrox launches new Centrifugal Slurry Pump**

Flowrox has launched a new heavy-duty CF-S horizontal centrifugal pump that is designed for continuous pumping of highly abrasive and dense slurries. The CF-S pump is ideal for grinding mill discharge, hydrocyclone feed, minerals processing, tailings, sugar processing and other industrial applications.

The CF-S pump provides ideal duty points with flows from as low as 2.3 m3/h to over 4 000 m3/h. A single Flowrox CF-S centrifugal pump can reach heads in excess of 76 m and provides a good balance between efficiency and wear.

The construction of the Flowrox CF-S pump is based on a split-case and has available a range of liner material options for optimal performance.

Flowrox Digital Services (supporting Industrial Internet of Things, IIoT) are optional features which increase Flowrox CF-S pump’s productivity through optimization and online predictability.

The horizontal CF-S pump is the first in a range of high-quality centrifugal pumps which Flowrox is launching.

## For more information,

## **Martti Lahtinen**, Business Line Director, Mining, Minerals Processing, Metallurgy martti.lahtinen@flowrox.com

*Flowrox is a global supplier of flow control, pumping, filtration and environmental engineering solutions, as well as intelligent applications and automation systems. Flowrox focuses on solving problems related to the shut-off, control, pumping and separation of abrasive, corrosive, and other demanding media, and also provides IIoT solutions for various process industry applications, in particular in the mining and mineral sector and energy and environmental sector.*

*Flowrox has subsidiaries in the United States, Australia, South Africa, Russia, Sweden, Chile and China, as well as a total of over 220 sales representatives in 81 countries.*