********M12 T-distributors for data transmission**

New M12 T-distributors for data transmission are available from Phoenix Contact. The T-distributors for PROFIBUS have 360° shielding and ensure safe data transmission and distribution.

They enable high data rates of up to 12 Mbps. An A-coded T-distributor for CANopen® completes the product range.

All T-distributors can be fixed with no rotation in two mounting holes. M12 knurls can still be turned, even when they are mounted. A variant with a fixed knurl is available for Profibus. It also simplifies connection of moulded cables with a knurl that can be turned. Thanks to the Speedcon fast locking system, all T-distributors are installed quickly. This ensures that the connection time is reduced by 90 percent for the user. The distributors are available in the IP65 and IP67 degrees of protection and are oil-resistant.

**ENDS**

**September 2017**

**PR4950GB**

Phoenix Contact Ltd

Halesfield 13

Telford

Shropshire

TF7 4PG

Tel: 0845 881 2222

Fax: 0845 881 2211

[www.phoenixcontact.co.uk](http://www.phoenixcontact.co.uk)

info@phoenixcontact.co.uk

**For news updates from Phoenix Contact visit:**

**Phoenix Contact Press Room** – http://www.mynewsdesk.com/uk/phoenix-contact-uk

**Twitter** - @phoenixcontactu

**YouTube** – Phoenix Contact UK

**Blog** – www.phoenixcontact.co.uk/blog

**LinkedIn** – www.linkedin.com/company/phoenix-contact-uk