**Unmanaged switches with IP67 degree of protection**

# The new unmanaged switches for field installation expand the product range of Ethernet switches from Phoenix Contact. The new 1608 and 1708 variants of the FL Switch 1000 product family feature the IP65/IP66/IP67 degrees of protection and make it easier to integrate distributed sensors, actuators, cameras, and I/O stations into the network.

# The rugged housing design provides nearly unlimited options for choosing a mounting position. The flexible M12 connection technology lets the user choose between using classic M12 connectors with screw connection and the M12 PUSH-PULL fast locking system from Phoenix Contact. The unmanaged switches support the Quality of Service (QoS) functionalities of the FL Switch 1000 product series for customary use of automation protocol prioritization.

**ENDS**

# PR5361GB

August 2021

Phoenix Contact Ltd

Halesfield 13

Telford

Shropshire

TF7 4PG

Tel: 0845 881 2222

Fax: 0845 881 2211

[www.phoenixcontact.co.uk](http://www.phoenixcontact.co.uk)

info@phoenixcontact.co.uk

**For news updates from Phoenix Contact visit:**

**Phoenix Contact Press Room** – http://www.mynewsdesk.com/uk/phoenix-contact-uk

**Twitter** - @phoenixcontactu

**YouTube** – Phoenix Contact

**Blog** – www.phoenixcontact.co.uk/blog

**LinkedIn** – www.linkedin.com/company/phoenix-contact

For further information on this press release please contact:

Phoenix Contact Ltd, Halesfield 13, Telford, TF7 4PG.

marketing@phoenixcontact.co.uk