******Industrial UV LED color printer**

The new Phoenix Contact Bluemark ID printer generation is the all-in-one solution for professional marking.

As a CMYK printer, this environmentally friendly printer is not limited to monochrome marking. It also utilises all the advantages offered by colour printing. The innovative UV LED printing process creates high quality markers that can be used right away. You can use the scalable printing resolution to adapt the fluid consumption and printing speed based on the application. The integrated marking software supports and monitors the printing process. The direct entry of print data using the 7“ multi-colour touch display and the easy menu navigation ensure intuitive operation.

In addition to plastic and aluminium, the printer also marks marking materials made of stainless steel. The material portfolio with over 1350 marking materials offers the user a high level of flexibility. The optionally selectable front feed enables flexible material assembly. As such, the colour printer can also use ANSI A format paper. The automatic offloading function enables the processing of more than 14,000 markers per hour (colour printing) and 21,000 markers (monochrome printing) per hour. The printer can be integrated into existing system structures using integrated interfaces.

 **ENDS**

**April 2018**

**PR5022GB**

Phoenix Contact Ltd

Halesfield 13

Telford

Shropshire

TF7 4PG

Tel: 0845 881 2222

Fax: 0845 881 2211

[www.phoenixcontact.co.uk](http://www.phoenixcontact.co.uk)

info@phoenixcontact.co.uk

**For news updates from Phoenix Contact visit:**

**Phoenix Contact Press Room** – http://www.mynewsdesk.com/uk/phoenix-contact-uk

**Twitter** - @phoenixcontactu

**YouTube** – Phoenix Contact UK

**Blog** – www.phoenixcontact.co.uk/blog

**LinkedIn** – www.linkedin.com/company/phoenix-contact-uk