****

**Space- and time-saving sensor connection**

# The new, only 3.5 mm-wide PTIO 1,5 initiator/actuator terminal blocks from Phoenix Contact are particularly suitable for wiring modern machine controls. They offer the option to connect sensors with two signal outputs in a space-saving manner.

# All bipolar sensors, including PE, are wired in just one terminal block. With their tool-free Push-in direct connection technology, PTIO terminal blocks also enable time-saving conductor connection.

# Flexible feed-in is enabled by identically shaped power terminals. The plus/minus potential is distributed with bridges, which considerably reduces wiring effort. Clarity of overview can be obtained by clearly marking all levels. With the standard accessories of the Clipline complete terminal blocks, warehousing costs can also be reduced.

# Ends

# PR5225GB

January 2020

Phoenix Contact Ltd

Halesfield 13

Telford

Shropshire

TF7 4PG

Tel: 0845 881 2222

Fax: 0845 881 2211

[www.phoenixcontact.co.uk](http://www.phoenixcontact.co.uk)

info@phoenixcontact.co.uk

**For news updates from Phoenix Contact visit:**

**Phoenix Contact Press Room** – http://www.mynewsdesk.com/uk/phoenix-contact-uk

**Twitter** - @phoenixcontactu

**YouTube** – Phoenix Contact UK

**Blog** – www.phoenixcontact.co.uk/blog

**LinkedIn** – www.linkedin.com/company/phoenix-contact-uk

For further information on this press release please contact:

Phoenix Contact Ltd, Halesfield 13, Telford, TF7 4PG.

marketing@phoenixcontact.co.uk