**Knife disconnect terminal blocks with colour-coded disconnect lever**



The knife disconnect terminal blocks from Phoenix Contact enable you to detect malfunctions and carry out inspections while the system is de-energised. The new UT…-MTL terminal blocks with screw connection have a disconnect lever which is actuated without tools. This enables the circuits to be separated easily. The disconnect lever locks in the end positions.

The disconnect point is also colour-coded to make it easy to identify. The disconnect lever is available in orange, white, and red. Product versions with test socket screws are available for convenient measurement. This enables a measuring device to be looped in upstream or downstream of the disconnect point. The double function shaft enables potentials to be distributed easily using plug-in bridges.

The new knife disconnect terminal blocks are suitable for conductors up to 10 mm². The uniform Clipline complete system accessories reduce logistics costs for the terminal blocks.

**ENDS**

**June 2016**

**PR4864GB**

Phoenix Contact Ltd

Halesfield 13

Telford

Shropshire

TF7 4PG

Tel: 0845 881 2222

Fax: 0845 881 2211

[www.phoenixcontact.co.uk](http://www.phoenixcontact.co.uk)

[info@phoenixcontact.co.uk](mailto:info@phoenixcontact.co.uk)

**For news updates from Phoenix Contact visit:**

**Phoenix Contact Press Room** – http://www.mynewsdesk.com/uk/phoenix-contact-uk

**Twitter** - @phoenixcontactu

**YouTube** – Phoenix Contact UK

**Blog** – www.phoenixcontact.co.uk/blog

**LinkedIn** – www.linkedin.com/company/phoenix-contact-uk