******High-position Push-in contact inserts for heavy-duty connectors**

The new modular 12-position Push-in contact inserts from Phoenix Contact can be used to easily connect up to six modules with a total of 72 signal contacts in a B24 connector.

The extremely compact terminal chamber saves space and enables a high packing density. Previously, this was only possible using a traditional crimp connection. Conductors of up to 1.5 mm² are installed without tools using the Push-in connection. They feature secure signal transmission up to 10 A and 250 V. You can combine the new inserts with additional modules to create an individual connector. This creates a highly compact modular interface in the housing. The pin and socket versions fit inside the series B housing and are plug-compatible with commercially available crimp connection modules.

**ENDS**

**May 2018**

**PR5030GB**

Phoenix Contact Ltd

Halesfield 13

Telford

Shropshire

TF7 4PG

Tel: 0845 881 2222

Fax: 0845 881 2211

[www.phoenixcontact.co.uk](http://www.phoenixcontact.co.uk)

info@phoenixcontact.co.uk

**For news updates from Phoenix Contact visit:**

**Phoenix Contact Press Room** – http://www.mynewsdesk.com/uk/phoenix-contact-uk

**Twitter** - @phoenixcontactu

**YouTube** – Phoenix Contact UK

**Blog** – www.phoenixcontact.co.uk/blog

**LinkedIn** – www.linkedin.com/company/phoenix-contact-uk