********Housing for heavy-duty connectors in a space-saving design**

For the protection of interfaces in a particularly narrow design, Phoenix Contact is now offering the new Heavycon Standard housing in sizes D15, D25, and D50.

They consist of high-quality corrosion-resistant die-cast aluminium and are reliably sealed up to IP67 protection. Thanks to their conductive surfaces and seals, the housings are also suitable for EMC applications. The housings can be mounted and maintained quickly and easily. They offer complete plug-in and mounting compatibility with the industry standard.

All contact inserts from the A10 and A16 series can be used in the new housings. The D50 housings with double-locking latches each accommodate two inserts side by side.

**ENDS**

**June 2017**

**PR4948GB**

Phoenix Contact Ltd

Halesfield 13

Telford

Shropshire

TF7 4PG

Tel: 0845 881 2222

Fax: 0845 881 2211

[www.phoenixcontact.co.uk](http://www.phoenixcontact.co.uk)

[info@phoenixcontact.co.uk](mailto:info@phoenixcontact.co.uk)

**For news updates from Phoenix Contact visit:**

**Phoenix Contact Press Room** – http://www.mynewsdesk.com/uk/phoenix-contact-uk

**Twitter** - @phoenixcontactu

**YouTube** – Phoenix Contact UK

**Blog** – www.phoenixcontact.co.uk/blog

**LinkedIn** – www.linkedin.com/company/phoenix-contact-uk